The following is a list of essential equipment to be carried on the main service vehicle(s). All employees should be trained in the use of specialized equipment such as the line tracer and the sounding equipment.

Fill out this checklist at the end of each month, checking the condition of all the equipment and replacing equipment as required.

Date:

**ITEM** **CONDITION**

2 SHOVELS Excellent Fair Replace

2 PICKS Excellent Fair Replace

VALVE KEYS Excellent Fair Replace

CURB STOP KEYS Excellent Fair Replace

PIPE WRENCHES Excellent Fair Replace

PIPE COVERS Excellent Fair Replace

SCREW DRIVERS Excellent Fair Replace

HOGGER FOR CLEANING CURB STOPS Excellent Fair Replace

METAL DETECTOR Excellent Fair Replace

LOCATOR (VALVE OR CURB STOPS) Excellent Fair Replace

LINE TRACER (PVC, COPPER, IRON, STEEL, CABLE) Excellent Fair Replace

SOUNDING EQUIPMENT Excellent Fair Replace

CHLORINE TEST KIT Excellent Fair Replace

HYDRANT VALVE WRENCH Excellent Fair Replace

TOOL TO REMOVE TOP OF HYDRANT Excellent Fair Replace

STETHISCOPE TO HEAR LEAKS IN SERVICE LINE Excellent Fair Replace

WRENCH FOR TAKING OFF TOP OF CURB STOPS Excellent Fair Replace

GAS CUT OFF SAW Excellent Fair Replace

PIPE CUTTERS Excellent Fair Replace

PUSH BAR Excellent Fair Replace

ELECTRIC PUMP FOR HYDRANTS Excellent Fair Replace

DIAMETER TAPE Excellent Fair Replace

Excellent Fair Replace

Excellent Fair Replace