The following is a list of essential equipment to be carried on the main service vehicle(s). All employees should be trained in the use of specialized equipment such as the line tracer and the sounding equipment.

Fill out this checklist at the end of each month, checking the condition of all the equipment and replacing equipment as required.

Date:

**ITEM** **CONDITION**

 2 SHOVELS Excellent Fair Replace

 2 PICKS Excellent Fair Replace

 VALVE KEYS Excellent Fair Replace

 CURB STOP KEYS Excellent Fair Replace

 PIPE WRENCHES Excellent Fair Replace

 PIPE COVERS Excellent Fair Replace

 SCREW DRIVERS Excellent Fair Replace

 HOGGER FOR CLEANING CURB STOPS Excellent Fair Replace

 METAL DETECTOR Excellent Fair Replace

 LOCATOR (VALVE OR CURB STOPS) Excellent Fair Replace

 LINE TRACER (PVC, COPPER, IRON, STEEL, CABLE) Excellent Fair Replace

 SOUNDING EQUIPMENT Excellent Fair Replace

 CHLORINE TEST KIT Excellent Fair Replace

 HYDRANT VALVE WRENCH Excellent Fair Replace

 TOOL TO REMOVE TOP OF HYDRANT Excellent Fair Replace

 STETHISCOPE TO HEAR LEAKS IN SERVICE LINE Excellent Fair Replace

 WRENCH FOR TAKING OFF TOP OF CURB STOPS Excellent Fair Replace

 GAS CUT OFF SAW Excellent Fair Replace

 PIPE CUTTERS Excellent Fair Replace

 PUSH BAR Excellent Fair Replace

 ELECTRIC PUMP FOR HYDRANTS Excellent Fair Replace

 DIAMETER TAPE Excellent Fair Replace

 Excellent Fair Replace

 Excellent Fair Replace